# Static Call Graph for image .\output\stmf10x-demo.axf

#<CALLGRAPH># ARM Linker, 5060422: Last Updated: Mon Nov 20 12:26:44 2017

### Maximum Stack Usage = 576 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ BMP180_test ⇒ BMP_UncompemstatedToTrue ⇒ BMP_Read_UP ⇒ BMP_ReadTwoByte ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- PendSV_Handler ⇒ PendSV_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x.o(.text) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from usart.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from usart.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from usart.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from usart.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_hd.o(.text)
  - _get_lc_ctype from lc_ctype_c.o(locale$$code) referenced from rt_ctype_table.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - _sputc from _sputc.o(.text) referenced from c89vsprintf.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_n (Thumb, 0 bytes, Stack size unknown bytes, _printf_n.o(.ARM.Collect$$_printf_percent$$00000001))
  [Calls]

  - >> _printf_charcount

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_p (Thumb, 0 bytes, Stack size unknown bytes, _printf_p.o(.ARM.Collect$$_printf_percent$$00000002))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_p ⇒ _printf_hex_ptr ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_hex_ptr

  _printf_f (Thumb, 0 bytes, Stack size unknown bytes, _printf_f.o(.ARM.Collect$$_printf_percent$$00000003))
  [Stack]

  - Max Depth = 320 + Unknown Stack Size
  - Call Chain = _printf_f ⇒ _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec

  _printf_e (Thumb, 0 bytes, Stack size unknown bytes, _printf_e.o(.ARM.Collect$$_printf_percent$$00000004))
  [Stack]

  - Max Depth = 320 + Unknown Stack Size
  - Call Chain = _printf_e ⇒ _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec

  _printf_g (Thumb, 0 bytes, Stack size unknown bytes, _printf_g.o(.ARM.Collect$$_printf_percent$$00000005))
  [Stack]

  - Max Depth = 320 + Unknown Stack Size
  - Call Chain = _printf_g ⇒ _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec

  _printf_a (Thumb, 0 bytes, Stack size unknown bytes, _printf_a.o(.ARM.Collect$$_printf_percent$$00000006))

  _printf_ll (Thumb, 0 bytes, Stack size unknown bytes, _printf_ll.o(.ARM.Collect$$_printf_percent$$00000007))

  _printf_i (Thumb, 0 bytes, Stack size unknown bytes, _printf_i.o(.ARM.Collect$$_printf_percent$$00000008))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_i ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_u (Thumb, 0 bytes, Stack size unknown bytes, _printf_u.o(.ARM.Collect$$_printf_percent$$0000000A))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_u ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_o (Thumb, 0 bytes, Stack size unknown bytes, _printf_o.o(.ARM.Collect$$_printf_percent$$0000000B))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_o ⇒ _printf_int_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_oct

  _printf_x (Thumb, 0 bytes, Stack size unknown bytes, _printf_x.o(.ARM.Collect$$_printf_percent$$0000000C))
  [Stack]

  - Max Depth = 80 + Unknown Stack Size
  - Call Chain = _printf_x ⇒ _printf_int_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_hex

  _printf_lli (Thumb, 0 bytes, Stack size unknown bytes, _printf_lli.o(.ARM.Collect$$_printf_percent$$0000000D))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_lli ⇒ _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_dec

  _printf_lld (Thumb, 0 bytes, Stack size unknown bytes, _printf_lld.o(.ARM.Collect$$_printf_percent$$0000000E))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_lld ⇒ _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_dec

  _printf_llu (Thumb, 0 bytes, Stack size unknown bytes, _printf_llu.o(.ARM.Collect$$_printf_percent$$0000000F))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_llu ⇒ _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_dec

  _printf_llo (Thumb, 0 bytes, Stack size unknown bytes, _printf_llo.o(.ARM.Collect$$_printf_percent$$00000010))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = _printf_llo ⇒ _printf_ll_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_ll_oct

  _printf_llx (Thumb, 0 bytes, Stack size unknown bytes, _printf_llx.o(.ARM.Collect$$_printf_percent$$00000011))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_llx ⇒ _printf_ll_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_ll_hex

  _printf_l (Thumb, 0 bytes, Stack size unknown bytes, _printf_l.o(.ARM.Collect$$_printf_percent$$00000012))

  _printf_c (Thumb, 0 bytes, Stack size unknown bytes, _printf_c.o(.ARM.Collect$$_printf_percent$$00000013))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = _printf_c ⇒ _printf_char ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_char

  _printf_s (Thumb, 0 bytes, Stack size unknown bytes, _printf_s.o(.ARM.Collect$$_printf_percent$$00000014))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = _printf_s ⇒ _printf_string ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_string

  _printf_lc (Thumb, 0 bytes, Stack size unknown bytes, _printf_lc.o(.ARM.Collect$$_printf_percent$$00000015))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = _printf_lc ⇒ _printf_wchar ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_wchar

  _printf_ls (Thumb, 0 bytes, Stack size unknown bytes, _printf_ls.o(.ARM.Collect$$_printf_percent$$00000016))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = _printf_ls ⇒ _printf_wstring ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_wstring

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_common (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))
  [Calls]

  - >> __rt_locale

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_2 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000012))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init_lc_ctype_2 ⇒ _get_lc_ctype
  [Calls]
  - >> _get_lc_ctype

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_2 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000016))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init_lc_numeric_2 ⇒ _get_lc_numeric
  [Calls]
  - >> _get_lc_numeric

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 576 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ BMP180_test ⇒ BMP_UncompemstatedToTrue ⇒ BMP_Read_UP ⇒ BMP_ReadTwoByte ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  SystemCoreClockUpdate (Thumb, 142 bytes, Stack size 8 bytes, system_stm32f10x.o(.text), UNUSED)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_hd.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> Hardware_Init

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> Usart4_Init
  - >> Usart3_Init
  - >> Usart2_Init
  - >> Usart1_Init

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 172 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 20 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> IIC_1750_Init
  - >> IIC_Init
  - >> Usart4_Init
  - >> Usart3_Init
  - >> Usart2_Init
  - >> Usart1_Init
  - >> Key_Init
  - >> Beep_Init
  - >> Led_Init

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> IIC_1750_RecvByte
  - >> IIC_1750_WaitAck
  - >> IIC_WaitAck
  - >> IIC_RecvByte
  - >> KeyScan

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> IIC_1750_RecvByte
  - >> IIC_1750_SendByte
  - >> IIC_1750_NAck
  - >> IIC_1750_Ack
  - >> IIC_1750_WaitAck
  - >> IIC_1750_Stop
  - >> IIC_1750_Start
  - >> IIC_1750_Init
  - >> IIC_Init
  - >> IIC_WaitAck
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_SendByte
  - >> IIC_RecvByte
  - >> IIC_NAck
  - >> IIC_Ack

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> IIC_1750_RecvByte
  - >> IIC_1750_SendByte
  - >> IIC_1750_NAck
  - >> IIC_1750_Ack
  - >> IIC_1750_WaitAck
  - >> IIC_1750_Stop
  - >> IIC_1750_Start
  - >> IIC_WaitAck
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_SendByte
  - >> IIC_RecvByte
  - >> IIC_NAck
  - >> IIC_Ack

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> Beep_Set
  - >> Led1_Set
  - >> Led2_Set
  - >> Led3_Set
  - >> Led4_Set

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 138 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EXTILineConfig (Thumb, 66 bytes, Stack size 12 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 64 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 70 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 56 bytes, Stack size 8 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 50 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  RCC_AHBPeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> IIC_1750_Init
  - >> IIC_Init
  - >> Usart4_Init
  - >> Usart3_Init
  - >> Usart2_Init
  - >> Usart1_Init
  - >> Key_Init
  - >> Beep_Init
  - >> Led_Init

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> Usart4_Init
  - >> Usart3_Init
  - >> Usart2_Init

  RCC_APB2PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> USART_DeInit
  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> USART_DeInit

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  USART_DeInit (Thumb, 134 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  USART_Init (Thumb, 210 bytes, Stack size 56 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> Usart4_Init
  - >> Usart3_Init
  - >> Usart2_Init
  - >> Usart1_Init

  USART_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 34 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> Usart4_Init
  - >> Usart3_Init
  - >> Usart2_Init
  - >> Usart1_Init

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> Usart4_Init
  - >> Usart3_Init
  - >> Usart2_Init
  - >> Usart1_Init

  USART_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetAddress (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> Usart_SendString
  - >> UsartPrintf

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> Usart_SendString
  - >> UsartPrintf

  USART_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> UART4_IRQHandler
  - >> USART3_IRQHandler
  - >> USART2_IRQHandler
  - >> USART1_IRQHandler

  USART_GetITStatus (Thumb, 84 bytes, Stack size 16 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> UART4_IRQHandler
  - >> USART3_IRQHandler
  - >> USART2_IRQHandler
  - >> USART1_IRQHandler

  USART_ClearITPendingBit (Thumb, 52 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  Led4_Set (Thumb, 38 bytes, Stack size 8 bytes, led.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Led4_Set
  [Calls]
  - >> GPIO_WriteBit
  [Called By]
  - >> Led_test
  - >> Led_Init

  Led3_Set (Thumb, 38 bytes, Stack size 8 bytes, led.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Led3_Set
  [Calls]
  - >> GPIO_WriteBit
  [Called By]
  - >> Led_test
  - >> Led_Init

  Led2_Set (Thumb, 38 bytes, Stack size 8 bytes, led.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Led2_Set
  [Calls]
  - >> GPIO_WriteBit
  [Called By]
  - >> Led_test
  - >> Led_Init

  Led1_Set (Thumb, 38 bytes, Stack size 8 bytes, led.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Led1_Set
  [Calls]
  - >> GPIO_WriteBit
  [Called By]
  - >> Led_test
  - >> Led_Init

  Led_Init (Thumb, 62 bytes, Stack size 8 bytes, led.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Led_Init ⇒ GPIO_Init
  [Calls]
  - >> Led1_Set
  - >> Led2_Set
  - >> Led3_Set
  - >> Led4_Set
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> Hardware_Init

  Led_test (Thumb, 78 bytes, Stack size 8 bytes, led.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Led_test ⇒ Led1_Set
  [Calls]
  - >> DelayXms
  - >> Led1_Set
  - >> Led2_Set
  - >> Led3_Set
  - >> Led4_Set
  [Called By]
  - >> main

  Delay_Init (Thumb, 48 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> Hardware_Init

  DelayUs (Thumb, 60 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> ADXL345_GetValue
  - >> ADXL345_Init
  - >> Read_BH1750
  - >> Cmd_Write_BH1750
  - >> I2C_1750_WriteBytes
  - >> IIC_1750_RecvByte
  - >> IIC_1750_SendByte
  - >> IIC_1750_NAck
  - >> IIC_1750_Ack
  - >> IIC_1750_WaitAck
  - >> IIC_1750_Stop
  - >> IIC_1750_Start
  - >> I2C_WriteBytes
  - >> IIC_WaitAck
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_SendByte
  - >> IIC_RecvByte
  - >> IIC_NAck
  - >> IIC_Ack
  - >> SHT20_GetValue

  DelayXms (Thumb, 66 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> BMP_Read_UP
  - >> BMP_Read_UT
  - >> BH1750_test
  - >> SHT20_GetValue
  - >> SHT2x_MeasureHM
  - >> Beep_test
  - >> DelayMs
  - >> Led_test

  DelayMs (Thumb, 60 bytes, Stack size 16 bytes, delay.o(.text), UNUSED)
  [Calls]

  - >> DelayXms

  Beep_Set (Thumb, 20 bytes, Stack size 8 bytes, beep.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Beep_Set
  [Calls]
  - >> GPIO_WriteBit
  [Called By]
  - >> Beep_test
  - >> Beep_Init

  Beep_Init (Thumb, 44 bytes, Stack size 8 bytes, beep.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Beep_Init ⇒ GPIO_Init
  [Calls]
  - >> Beep_Set
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> Hardware_Init

  Beep_test (Thumb, 30 bytes, Stack size 8 bytes, beep.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Beep_test ⇒ Beep_Set
  [Calls]
  - >> Beep_Set
  - >> DelayXms
  [Called By]
  - >> main

  Key_Init (Thumb, 38 bytes, Stack size 8 bytes, key.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Key_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> Hardware_Init

  KeyScan (Thumb, 32 bytes, Stack size 16 bytes, key.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = KeyScan
  [Calls]
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> Keyboard

  Keyboard (Thumb, 116 bytes, Stack size 8 bytes, key.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Keyboard ⇒ KeyScan
  [Calls]
  - >> KeyScan
  [Called By]
  - >> Key_test

  Key_test (Thumb, 68 bytes, Stack size 8 bytes, key.o(.text))
  [Stack]

  - Max Depth = 456 + Unknown Stack Size
  - Call Chain = Key_test ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> UsartPrintf
  - >> Keyboard
  [Called By]
  - >> main

  SHT20_reset (Thumb, 14 bytes, Stack size 8 bytes, sht20.o(.text))
  [Stack]

  - Max Depth = 488 + Unknown Stack Size
  - Call Chain = SHT20_reset ⇒ I2C_WriteByte ⇒ IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> I2C_WriteByte
  [Called By]
  - >> SHT20_GetValue

  SHT20_read_user_reg (Thumb, 22 bytes, Stack size 8 bytes, sht20.o(.text))
  [Stack]

  - Max Depth = 488 + Unknown Stack Size
  - Call Chain = SHT20_read_user_reg ⇒ I2C_ReadByte ⇒ IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> I2C_ReadByte
  [Called By]
  - >> SHT20_GetValue

  SHT2x_CheckCrc (Thumb, 74 bytes, Stack size 16 bytes, sht20.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SHT2x_CheckCrc
  [Called By]
  - >> SHT2x_MeasureHM

  SHT2x_CalcTemperatureC (Thumb, 60 bytes, Stack size 40 bytes, sht20.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = SHT2x_CalcTemperatureC ⇒ __aeabi_d2f
  [Calls]
  - >> __aeabi_dadd
  - >> __aeabi_d2f
  - >> __aeabi_ui2f
  - >> __aeabi_f2d
  - >> __aeabi_dmul
  [Called By]
  - >> SHT2x_MeasureHM

  SHT2x_CalcRH (Thumb, 60 bytes, Stack size 40 bytes, sht20.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = SHT2x_CalcRH ⇒ __aeabi_dsub
  [Calls]
  - >> __aeabi_dsub
  - >> __aeabi_d2f
  - >> __aeabi_ui2f
  - >> __aeabi_f2d
  - >> __aeabi_dmul
  [Called By]
  - >> SHT2x_MeasureHM

  SHT2x_MeasureHM (Thumb, 208 bytes, Stack size 32 bytes, sht20.o(.text))
  [Stack]

  - Max Depth = 488 + Unknown Stack Size
  - Call Chain = SHT2x_MeasureHM ⇒ IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_WaitAck
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_SendByte
  - >> IIC_RecvByte
  - >> IIC_NAck
  - >> IIC_Ack
  - >> SHT2x_CalcRH
  - >> SHT2x_CalcTemperatureC
  - >> SHT2x_CheckCrc
  - >> DelayXms
  - >> __aeabi_f2uiz
  [Called By]
  - >> SHT20_GetValue

  SHT20_GetValue (Thumb, 106 bytes, Stack size 8 bytes, sht20.o(.text))
  [Stack]

  - Max Depth = 496 + Unknown Stack Size
  - Call Chain = SHT20_GetValue ⇒ SHT2x_MeasureHM ⇒ IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_SpeedCtl
  - >> I2C_WriteByte
  - >> SHT2x_MeasureHM
  - >> SHT20_read_user_reg
  - >> SHT20_reset
  - >> DelayUs
  - >> DelayXms
  [Called By]
  - >> SHT20_test

  SHT20_test (Thumb, 52 bytes, Stack size 16 bytes, sht20.o(.text))
  [Stack]

  - Max Depth = 512 + Unknown Stack Size
  - Call Chain = SHT20_test ⇒ SHT20_GetValue ⇒ SHT2x_MeasureHM ⇒ IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> SHT20_GetValue
  - >> UsartPrintf
  - >> __aeabi_f2d
  [Called By]
  - >> main

  Usart1_Init (Thumb, 166 bytes, Stack size 32 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = Usart1_Init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> NVIC_Init
  [Called By]
  - >> Hardware_Init

  Usart2_Init (Thumb, 162 bytes, Stack size 32 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = Usart2_Init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_Init
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> NVIC_Init
  [Called By]
  - >> Hardware_Init

  Usart3_Init (Thumb, 164 bytes, Stack size 32 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = Usart3_Init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_Init
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> NVIC_Init
  [Called By]
  - >> Hardware_Init

  Usart4_Init (Thumb, 164 bytes, Stack size 32 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = Usart4_Init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_ITConfig
  - >> USART_Cmd
  - >> USART_Init
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  - >> NVIC_Init
  [Called By]
  - >> Hardware_Init

  Usart_SendString (Thumb, 50 bytes, Stack size 24 bytes, usart.o(.text), UNUSED)
  [Calls]

  - >> USART_GetFlagStatus
  - >> USART_SendData

  UsartPrintf (Thumb, 68 bytes, Stack size 328 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 448 + Unknown Stack Size
  - Call Chain = UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __c89vsprintf
  - >> USART_GetFlagStatus
  - >> USART_SendData
  [Called By]
  - >> main
  - >> BMP180_test
  - >> ADXL345_GetValue
  - >> Convert_BH1750
  - >> IIC_1750_WaitAck
  - >> USART_test
  - >> IIC_WaitAck
  - >> SHT20_test
  - >> Key_test

  USART1_IRQHandler (Thumb, 62 bytes, Stack size 8 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_GetITStatus
  - >> USART_ClearFlag
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 62 bytes, Stack size 8 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART2_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_GetITStatus
  - >> USART_ClearFlag
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 62 bytes, Stack size 8 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART3_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_GetITStatus
  - >> USART_ClearFlag
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 62 bytes, Stack size 8 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART4_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_GetITStatus
  - >> USART_ClearFlag
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USART_test (Thumb, 218 bytes, Stack size 8 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 456 + Unknown Stack Size
  - Call Chain = USART_test ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __aeabi_memclr
  - >> UsartPrintf
  [Called By]
  - >> main

  IIC_SpeedCtl (Thumb, 6 bytes, Stack size 0 bytes, i2c.o(.text))
  [Called By]

  - >> ADXL345_GetValue
  - >> IIC_Init
  - >> SHT20_GetValue

  IIC_Init (Thumb, 60 bytes, Stack size 8 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = IIC_Init ⇒ GPIO_Init
  [Calls]
  - >> IIC_SpeedCtl
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> Hardware_Init

  IIC_Start (Thumb, 52 bytes, Stack size 8 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Start
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> I2C_ReadBytes
  - >> I2C_WriteBytes
  - >> I2C_WriteByte
  - >> I2C_ReadByte
  - >> SHT2x_MeasureHM

  IIC_Stop (Thumb, 52 bytes, Stack size 8 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Stop
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> I2C_ReadBytes
  - >> I2C_WriteBytes
  - >> IIC_WaitAck
  - >> I2C_WriteByte
  - >> I2C_ReadByte
  - >> SHT2x_MeasureHM

  IIC_WaitAck (Thumb, 92 bytes, Stack size 8 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 456 + Unknown Stack Size
  - Call Chain = IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_Stop
  - >> UsartPrintf
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> I2C_ReadBytes
  - >> I2C_WriteBytes
  - >> I2C_WriteByte
  - >> I2C_ReadByte
  - >> SHT2x_MeasureHM

  IIC_Ack (Thumb, 52 bytes, Stack size 8 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_Ack
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> I2C_ReadBytes
  - >> SHT2x_MeasureHM

  IIC_NAck (Thumb, 52 bytes, Stack size 8 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_NAck
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> I2C_ReadBytes
  - >> I2C_ReadByte
  - >> SHT2x_MeasureHM

  IIC_SendByte (Thumb, 86 bytes, Stack size 16 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_SendByte
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> I2C_ReadBytes
  - >> I2C_WriteBytes
  - >> I2C_WriteByte
  - >> I2C_ReadByte
  - >> SHT2x_MeasureHM

  IIC_RecvByte (Thumb, 78 bytes, Stack size 16 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_RecvByte
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> I2C_ReadBytes
  - >> I2C_ReadByte
  - >> SHT2x_MeasureHM

  I2C_WriteByte (Thumb, 92 bytes, Stack size 24 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 480 + Unknown Stack Size
  - Call Chain = I2C_WriteByte ⇒ IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_WaitAck
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_SendByte
  [Called By]
  - >> ADXL345_Init
  - >> SHT20_GetValue
  - >> SHT20_reset

  I2C_ReadByte (Thumb, 106 bytes, Stack size 24 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 480 + Unknown Stack Size
  - Call Chain = I2C_ReadByte ⇒ IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_WaitAck
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_SendByte
  - >> IIC_RecvByte
  - >> IIC_NAck
  [Called By]
  - >> ADXL345_GetValue
  - >> ADXL345_Init
  - >> SHT20_read_user_reg

  I2C_WriteBytes (Thumb, 116 bytes, Stack size 24 bytes, i2c.o(.text), UNUSED)
  [Calls]

  - >> IIC_WaitAck
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_SendByte
  - >> DelayUs

  I2C_ReadBytes (Thumb, 136 bytes, Stack size 24 bytes, i2c.o(.text))
  [Stack]

  - Max Depth = 480 + Unknown Stack Size
  - Call Chain = I2C_ReadBytes ⇒ IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_WaitAck
  - >> IIC_Stop
  - >> IIC_Start
  - >> IIC_SendByte
  - >> IIC_RecvByte
  - >> IIC_NAck
  - >> IIC_Ack
  [Called By]
  - >> ADXL345_GetValue

  IIC_1750_SpeedCtl (Thumb, 6 bytes, Stack size 0 bytes, bh1750.o(.text))
  [Called By]

  - >> IIC_1750_Init

  IIC_1750_Init (Thumb, 66 bytes, Stack size 8 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = IIC_1750_Init ⇒ GPIO_Init
  [Calls]
  - >> IIC_1750_SpeedCtl
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> Hardware_Init

  IIC_1750_Start (Thumb, 60 bytes, Stack size 8 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_1750_Start
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> BMP_ReadTwoByte
  - >> Read_BH1750
  - >> Cmd_Write_BH1750
  - >> I2C_1750_ReadBytes
  - >> I2C_1750_WriteBytes
  - >> I2C_1750_ReadByte
  - >> I2C_1750_WriteByte

  IIC_1750_Stop (Thumb, 60 bytes, Stack size 8 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_1750_Stop
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> BMP_ReadTwoByte
  - >> Read_BH1750
  - >> Cmd_Write_BH1750
  - >> I2C_1750_ReadBytes
  - >> I2C_1750_WriteBytes
  - >> I2C_1750_ReadByte
  - >> I2C_1750_WriteByte
  - >> IIC_1750_WaitAck

  IIC_1750_WaitAck (Thumb, 100 bytes, Stack size 8 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 456 + Unknown Stack Size
  - Call Chain = IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_1750_Stop
  - >> UsartPrintf
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> BMP_ReadTwoByte
  - >> Read_BH1750
  - >> Cmd_Write_BH1750
  - >> I2C_1750_ReadBytes
  - >> I2C_1750_WriteBytes
  - >> I2C_1750_ReadByte
  - >> I2C_1750_WriteByte

  IIC_1750_Ack (Thumb, 60 bytes, Stack size 8 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_1750_Ack
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> BMP_ReadTwoByte
  - >> Read_BH1750
  - >> I2C_1750_ReadBytes

  IIC_1750_NAck (Thumb, 60 bytes, Stack size 8 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IIC_1750_NAck
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> BMP_ReadTwoByte
  - >> Read_BH1750
  - >> I2C_1750_ReadBytes
  - >> I2C_1750_ReadByte

  IIC_1750_SendByte (Thumb, 96 bytes, Stack size 16 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_1750_SendByte
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  [Called By]
  - >> BMP_ReadTwoByte
  - >> Read_BH1750
  - >> Cmd_Write_BH1750
  - >> I2C_1750_ReadBytes
  - >> I2C_1750_WriteBytes
  - >> I2C_1750_ReadByte
  - >> I2C_1750_WriteByte

  IIC_1750_RecvByte (Thumb, 86 bytes, Stack size 16 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IIC_1750_RecvByte
  [Calls]
  - >> DelayUs
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> BMP_ReadTwoByte
  - >> Read_BH1750
  - >> I2C_1750_ReadBytes
  - >> I2C_1750_ReadByte

  I2C_1750_WriteByte (Thumb, 92 bytes, Stack size 24 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 480 + Unknown Stack Size
  - Call Chain = I2C_1750_WriteByte ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_1750_SendByte
  - >> IIC_1750_WaitAck
  - >> IIC_1750_Stop
  - >> IIC_1750_Start
  [Called By]
  - >> BMP_Read_UP
  - >> BMP_Read_UT

  I2C_1750_ReadByte (Thumb, 106 bytes, Stack size 24 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 480 + Unknown Stack Size
  - Call Chain = I2C_1750_ReadByte ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_1750_RecvByte
  - >> IIC_1750_SendByte
  - >> IIC_1750_NAck
  - >> IIC_1750_WaitAck
  - >> IIC_1750_Stop
  - >> IIC_1750_Start
  [Called By]
  - >> BMP180_test

  I2C_1750_WriteBytes (Thumb, 116 bytes, Stack size 24 bytes, bh1750.o(.text), UNUSED)
  [Calls]

  - >> IIC_1750_SendByte
  - >> IIC_1750_WaitAck
  - >> IIC_1750_Stop
  - >> IIC_1750_Start
  - >> DelayUs

  I2C_1750_ReadBytes (Thumb, 168 bytes, Stack size 24 bytes, bh1750.o(.text), UNUSED)
  [Calls]

  - >> IIC_1750_RecvByte
  - >> IIC_1750_SendByte
  - >> IIC_1750_NAck
  - >> IIC_1750_Ack
  - >> IIC_1750_WaitAck
  - >> IIC_1750_Stop
  - >> IIC_1750_Start

  Cmd_Write_BH1750 (Thumb, 64 bytes, Stack size 8 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 464 + Unknown Stack Size
  - Call Chain = Cmd_Write_BH1750 ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_1750_SendByte
  - >> IIC_1750_WaitAck
  - >> IIC_1750_Stop
  - >> IIC_1750_Start
  - >> DelayUs
  [Called By]
  - >> Start_BH1750

  Start_BH1750 (Thumb, 22 bytes, Stack size 8 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 472 + Unknown Stack Size
  - Call Chain = Start_BH1750 ⇒ Cmd_Write_BH1750 ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> Cmd_Write_BH1750
  [Called By]
  - >> BH1750_test

  Read_BH1750 (Thumb, 66 bytes, Stack size 8 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 464 + Unknown Stack Size
  - Call Chain = Read_BH1750 ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_1750_RecvByte
  - >> IIC_1750_SendByte
  - >> IIC_1750_NAck
  - >> IIC_1750_Ack
  - >> IIC_1750_WaitAck
  - >> IIC_1750_Stop
  - >> IIC_1750_Start
  - >> DelayUs
  [Called By]
  - >> BH1750_test

  Convert_BH1750 (Thumb, 88 bytes, Stack size 24 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 472 + Unknown Stack Size
  - Call Chain = Convert_BH1750 ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __aeabi_ddiv
  - >> __aeabi_d2f
  - >> UsartPrintf
  - >> __aeabi_ui2f
  - >> __aeabi_f2d
  [Called By]
  - >> BH1750_test

  BH1750_test (Thumb, 22 bytes, Stack size 8 bytes, bh1750.o(.text))
  [Stack]

  - Max Depth = 480 + Unknown Stack Size
  - Call Chain = BH1750_test ⇒ Convert_BH1750 ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> Convert_BH1750
  - >> Read_BH1750
  - >> Start_BH1750
  - >> DelayXms
  [Called By]
  - >> main

  ADXL345_Init (Thumb, 166 bytes, Stack size 16 bytes, adxl345.o(.text))
  [Stack]

  - Max Depth = 496 + Unknown Stack Size
  - Call Chain = ADXL345_Init ⇒ I2C_WriteByte ⇒ IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> I2C_WriteByte
  - >> I2C_ReadByte
  - >> DelayUs
  [Called By]
  - >> Hardware_Init

  ADXL345_GetValue (Thumb, 272 bytes, Stack size 40 bytes, adxl345.o(.text))
  [Stack]

  - Max Depth = 520 + Unknown Stack Size
  - Call Chain = ADXL345_GetValue ⇒ I2C_ReadBytes ⇒ IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __aeabi_d2f
  - >> I2C_ReadBytes
  - >> IIC_SpeedCtl
  - >> I2C_ReadByte
  - >> UsartPrintf
  - >> DelayUs
  - >> __aeabi_i2f
  - >> __aeabi_f2d
  - >> __aeabi_dmul
  [Called By]
  - >> main

  BMP_ReadTwoByte (Thumb, 110 bytes, Stack size 24 bytes, bmp180.o(.text))
  [Stack]

  - Max Depth = 480 + Unknown Stack Size
  - Call Chain = BMP_ReadTwoByte ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> IIC_1750_RecvByte
  - >> IIC_1750_SendByte
  - >> IIC_1750_NAck
  - >> IIC_1750_Ack
  - >> IIC_1750_WaitAck
  - >> IIC_1750_Stop
  - >> IIC_1750_Start
  [Called By]
  - >> BMP_Read_UP
  - >> BMP_Read_UT
  - >> BMP_ReadCalibrationData

  BMP_ReadCalibrationData (Thumb, 114 bytes, Stack size 8 bytes, bmp180.o(.text))
  [Stack]

  - Max Depth = 488 + Unknown Stack Size
  - Call Chain = BMP_ReadCalibrationData ⇒ BMP_ReadTwoByte ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> BMP_ReadTwoByte
  [Called By]
  - >> BMP180_test

  BMP_Read_UT (Thumb, 32 bytes, Stack size 8 bytes, bmp180.o(.text))
  [Stack]

  - Max Depth = 488 + Unknown Stack Size
  - Call Chain = BMP_Read_UT ⇒ BMP_ReadTwoByte ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> BMP_ReadTwoByte
  - >> I2C_1750_WriteByte
  - >> DelayXms
  [Called By]
  - >> BMP_UncompemstatedToTrue

  BMP_Read_UP (Thumb, 34 bytes, Stack size 8 bytes, bmp180.o(.text))
  [Stack]

  - Max Depth = 488 + Unknown Stack Size
  - Call Chain = BMP_Read_UP ⇒ BMP_ReadTwoByte ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> BMP_ReadTwoByte
  - >> I2C_1750_WriteByte
  - >> DelayXms
  [Called By]
  - >> BMP_UncompemstatedToTrue

  BMP_UncompemstatedToTrue (Thumb, 442 bytes, Stack size 48 bytes, bmp180.o(.text))
  [Stack]

  - Max Depth = 536 + Unknown Stack Size
  - Call Chain = BMP_UncompemstatedToTrue ⇒ BMP_Read_UP ⇒ BMP_ReadTwoByte ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __aeabi_i2d
  - >> __aeabi_ddiv
  - >> __aeabi_drsub
  - >> __aeabi_d2f
  - >> BMP_Read_UP
  - >> BMP_Read_UT
  - >> pow
  - >> __aeabi_dmul
  [Called By]
  - >> BMP180_test

  BMP180_test (Thumb, 86 bytes, Stack size 40 bytes, bmp180.o(.text))
  [Stack]

  - Max Depth = 576 + Unknown Stack Size
  - Call Chain = BMP180_test ⇒ BMP_UncompemstatedToTrue ⇒ BMP_Read_UP ⇒ BMP_ReadTwoByte ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> BMP_UncompemstatedToTrue
  - >> BMP_ReadCalibrationData
  - >> I2C_1750_ReadByte
  - >> UsartPrintf
  - >> __aeabi_f2d
  [Called By]
  - >> main

  Hardware_Init (Thumb, 72 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 504 + Unknown Stack Size
  - Call Chain = Hardware_Init ⇒ ADXL345_Init ⇒ I2C_WriteByte ⇒ IIC_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> ADXL345_Init
  - >> IIC_1750_Init
  - >> IIC_Init
  - >> Usart4_Init
  - >> Usart3_Init
  - >> Usart2_Init
  - >> Usart1_Init
  - >> Key_Init
  - >> Beep_Init
  - >> Delay_Init
  - >> Led_Init
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> main

  main (Thumb, 80 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 576 + Unknown Stack Size
  - Call Chain = main ⇒ BMP180_test ⇒ BMP_UncompemstatedToTrue ⇒ BMP_Read_UP ⇒ BMP_ReadTwoByte ⇒ IIC_1750_WaitAck ⇒ UsartPrintf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> Hardware_Init
  - >> BMP180_test
  - >> ADXL345_GetValue
  - >> BH1750_test
  - >> USART_test
  - >> SHT20_test
  - >> UsartPrintf
  - >> Key_test
  - >> Beep_test
  - >> Led_test
  [Called By]
  - >> __rt_entry_main

  __c89vsprintf (Thumb, 32 bytes, Stack size 16 bytes, c89vsprintf.o(.text))
  [Stack]

  - Max Depth = 120 + Unknown Stack Size
  - Call Chain = __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _sputc
  - >> _printf_char_common
  [Called By]
  - >> UsartPrintf

  __aeabi_memclr (Thumb, 0 bytes, Stack size 0 bytes, rt_memclr.o(.text))
  [Called By]

  - >> USART_test

  __rt_memclr (Thumb, 68 bytes, Stack size 0 bytes, rt_memclr.o(.text), UNUSED)
  [Calls]

  - >> _memset_w

  _memset (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr.o(.text), UNUSED)

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __read_errno (Thumb, 10 bytes, Stack size 8 bytes, _rserrno.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_errno_addr

  __set_errno (Thumb, 12 bytes, Stack size 8 bytes, _rserrno.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __set_errno
  [Calls]
  - >> __aeabi_errno_addr
  [Called By]
  - >> sqrt
  - >> pow

  _printf_pre_padding (Thumb, 44 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_pre_padding
  [Called By]
  - >> _printf_fp_infnan
  - >> _printf_fp_dec_real
  - >> _printf_int_common
  - >> _printf_wctomb
  - >> _printf_str

  _printf_post_padding (Thumb, 34 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_post_padding
  [Called By]
  - >> _printf_fp_infnan
  - >> _printf_fp_dec_real
  - >> _printf_int_common
  - >> _printf_wctomb
  - >> _printf_str

  _printf_truncate_signed (Thumb, 18 bytes, Stack size 0 bytes, _printf_truncate.o(.text))
  [Called By]

  - >> _printf_int_dec

  _printf_truncate_unsigned (Thumb, 18 bytes, Stack size 0 bytes, _printf_truncate.o(.text))
  [Called By]

  - >> _printf_int_hex
  - >> _printf_int_oct
  - >> _printf_int_dec

  _printf_str (Thumb, 82 bytes, Stack size 16 bytes, _printf_str.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_cs_common

  _printf_int_dec (Thumb, 104 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  - >> _printf_truncate_unsigned
  - >> _printf_truncate_signed
  [Called By]
  - >> _printf_u
  - >> _printf_d
  - >> _printf_i

  _printf_charcount (Thumb, 40 bytes, Stack size 0 bytes, _printf_charcount.o(.text))
  [Called By]

  - >> _printf_n

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> __c89vsprintf

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, _sputc.o(.text))
  [Called By]

  - >> __c89vsprintf
  [Address Reference Count : 1]
  - c89vsprintf.o(.text)

  _printf_wctomb (Thumb, 182 bytes, Stack size 56 bytes, _printf_wctomb.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _wcrtomb
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_lcs_common

  _printf_longlong_dec (Thumb, 108 bytes, Stack size 24 bytes, _printf_longlong_dec.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  - >> _ll_udiv10
  [Called By]
  - >> _printf_llu
  - >> _printf_lld
  - >> _printf_lli

  _printf_longlong_oct (Thumb, 66 bytes, Stack size 8 bytes, _printf_oct_int_ll.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_ll_oct
  - >> _printf_int_oct

  _printf_int_oct (Thumb, 24 bytes, Stack size 8 bytes, _printf_oct_int_ll.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_int_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_oct
  - >> _printf_truncate_unsigned
  [Called By]
  - >> _printf_o

  _printf_ll_oct (Thumb, 12 bytes, Stack size 0 bytes, _printf_oct_int_ll.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_ll_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_oct
  [Called By]
  - >> _printf_llo

  _printf_longlong_hex (Thumb, 86 bytes, Stack size 16 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_hex_ptr
  - >> _printf_ll_hex
  - >> _printf_int_hex

  _printf_int_hex (Thumb, 28 bytes, Stack size 16 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = _printf_int_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_hex
  - >> _printf_truncate_unsigned
  [Called By]
  - >> _printf_x

  _printf_ll_hex (Thumb, 12 bytes, Stack size 0 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_ll_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_hex
  [Called By]
  - >> _printf_llx

  _printf_hex_ptr (Thumb, 18 bytes, Stack size 0 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_hex_ptr ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_hex
  [Called By]
  - >> _printf_p

  __printf (Thumb, 388 bytes, Stack size 40 bytes, __printf_flags_ss_wp.o(.text))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  - >> _is_digit
  [Called By]
  - >> _printf_char_common

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  __rt_memclr_w (Thumb, 78 bytes, Stack size 4 bytes, rt_memclr_w.o(.text), UNUSED)

  _memset_w (Thumb, 0 bytes, Stack size unknown bytes, rt_memclr_w.o(.text), UNUSED)
  [Called By]

  - >> __rt_memclr

  __aeabi_errno_addr (Thumb, 8 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text))
  [Called By]

  - >> __set_errno
  - >> __read_errno

  __errno$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  __rt_errno_addr$intlibspace (Thumb, 0 bytes, Stack size 0 bytes, rt_errno_addr_intlibspace.o(.text), UNUSED)

  _ll_udiv10 (Thumb, 138 bytes, Stack size 12 bytes, lludiv10.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = _ll_udiv10
  [Called By]
  - >> _fp_digits
  - >> _printf_longlong_dec

  _printf_int_common (Thumb, 178 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_longlong_hex
  - >> _printf_longlong_oct
  - >> _printf_longlong_dec
  - >> _printf_int_dec

  __lib_sel_fp_printf (Thumb, 2 bytes, Stack size 0 bytes, _printf_fp_dec.o(.text), UNUSED)

  _printf_fp_dec_real (Thumb, 620 bytes, Stack size 104 bytes, _printf_fp_dec.o(.text))
  [Stack]

  - Max Depth = 320
  - Call Chain = _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_infnan
  - >> __rt_locale
  - >> _fp_digits
  - >> __ARM_fpclassify
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_fp_dec

  _printf_cs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_str
  [Called By]
  - >> _printf_string
  - >> _printf_char

  _printf_char (Thumb, 16 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_char ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_c

  _printf_string (Thumb, 8 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_string ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_s

  _printf_lcs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_wchar.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_wctomb
  [Called By]
  - >> _printf_wstring
  - >> _printf_wchar

  _printf_wchar (Thumb, 16 bytes, Stack size 0 bytes, _printf_wchar.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = _printf_wchar ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_lcs_common
  [Called By]
  - >> _printf_lc

  _printf_wstring (Thumb, 8 bytes, Stack size 0 bytes, _printf_wchar.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = _printf_wstring ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_lcs_common
  [Called By]
  - >> _printf_ls

  _wcrtomb (Thumb, 64 bytes, Stack size 16 bytes, _wcrtomb.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> __rt_ctype_table
  [Called By]
  - >> _printf_wctomb

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  __rt_ctype_table (Thumb, 16 bytes, Stack size 8 bytes, rt_ctype_table.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __rt_ctype_table
  [Calls]
  - >> __rt_locale
  [Called By]
  - >> _wcrtomb

  __rt_locale (Thumb, 8 bytes, Stack size 0 bytes, rt_locale_intlibspace.o(.text))
  [Called By]

  - >> __rt_lib_init_lc_common
  - >> __rt_ctype_table
  - >> _printf_fp_dec_real

  _printf_fp_infnan (Thumb, 112 bytes, Stack size 24 bytes, _printf_fp_infnan.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_fp_infnan ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_fp_dec_real

  _btod_etento (Thumb, 216 bytes, Stack size 72 bytes, bigflt0.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _btod_emul
  - >> _btod_ediv
  [Called By]
  - >> _fp_digits

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  strcmp (Thumb, 128 bytes, Stack size 0 bytes, strcmpv7m.o(.text))
  [Called By]

  - >> _get_lc_ctype
  - >> _get_lc_numeric

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size 0 bytes, indicate_semi.o(.text), UNUSED)

  _btod_d2e (Thumb, 62 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e))
  [Calls]

  - >> _d2e_norm_op1
  [Called By]
  - >> _fp_digits

  _d2e_denorm_low (Thumb, 70 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e_denorm_low))
  [Called By]

  - >> _d2e_norm_op1

  _d2e_norm_op1 (Thumb, 96 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e_norm_op1))
  [Calls]

  - >> _d2e_denorm_low
  [Called By]
  - >> _btod_d2e

  __btod_div_common (Thumb, 696 bytes, Stack size 24 bytes, btod.o(CL$$btod_div_common))
  [Stack]

  - Max Depth = 24
  - Call Chain = __btod_div_common
  [Called By]
  - >> _btod_ediv

  _e2e (Thumb, 198 bytes, Stack size 24 bytes, btod.o(CL$$btod_e2e))
  [Stack]

  - Max Depth = 24
  - Call Chain = _e2e
  [Called By]
  - >> _btod_emul
  - >> _btod_ediv

  _btod_ediv (Thumb, 40 bytes, Stack size 24 bytes, btod.o(CL$$btod_ediv))
  [Stack]

  - Max Depth = 48
  - Call Chain = _btod_ediv ⇒ _e2e
  [Calls]
  - >> _e2e
  - >> __btod_div_common
  [Called By]
  - >> _btod_etento
  - >> _fp_digits

  _btod_emul (Thumb, 40 bytes, Stack size 24 bytes, btod.o(CL$$btod_emul))
  [Stack]

  - Max Depth = 48
  - Call Chain = _btod_emul ⇒ _e2e
  [Calls]
  - >> __btod_mult_common
  - >> _e2e
  [Called By]
  - >> _btod_etento
  - >> _fp_digits

  __btod_mult_common (Thumb, 580 bytes, Stack size 16 bytes, btod.o(CL$$btod_mult_common))
  [Stack]

  - Max Depth = 16
  - Call Chain = __btod_mult_common
  [Called By]
  - >> _btod_emul

  __ARM_fpclassify (Thumb, 40 bytes, Stack size 0 bytes, fpclassify.o(i.__ARM_fpclassify))
  [Called By]

  - >> _printf_fp_dec_real
  - >> pow

  __kernel_poly (Thumb, 170 bytes, Stack size 24 bytes, poly.o(i.__kernel_poly))
  [Stack]

  - Max Depth = 56
  - Call Chain = __kernel_poly ⇒ __aeabi_dmul
  [Calls]
  - >> __aeabi_dadd
  - >> __aeabi_dmul
  [Called By]
  - >> pow

  __mathlib_dbl_divzero (Thumb, 12 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_divzero))
  [Stack]

  - Max Depth = 32
  - Call Chain = __mathlib_dbl_divzero ⇒ __aeabi_ddiv
  [Calls]
  - >> __aeabi_ddiv
  [Called By]
  - >> pow

  __mathlib_dbl_infnan2 (Thumb, 4 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_infnan2))
  [Stack]

  - Max Depth = 16
  - Call Chain = __mathlib_dbl_infnan2 ⇒ __aeabi_dadd
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> pow

  __mathlib_dbl_invalid (Thumb, 12 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_invalid))
  [Stack]

  - Max Depth = 32
  - Call Chain = __mathlib_dbl_invalid ⇒ __aeabi_ddiv
  [Calls]
  - >> __aeabi_ddiv
  [Called By]
  - >> pow

  __mathlib_dbl_overflow (Thumb, 14 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_overflow))
  [Calls]

  - >> __ARM_scalbn
  [Called By]
  - >> pow

  __mathlib_dbl_underflow (Thumb, 10 bytes, Stack size 0 bytes, dunder.o(i.__mathlib_dbl_underflow))
  [Calls]

  - >> __ARM_scalbn
  [Called By]
  - >> pow

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, __printf_wp.o(i._is_digit))
  [Called By]

  - >> __printf

  pow (Thumb, 2512 bytes, Stack size 128 bytes, pow.o(i.pow))
  [Stack]

  - Max Depth = 192
  - Call Chain = pow ⇒ sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> __aeabi_i2d
  - >> __aeabi_ddiv
  - >> __aeabi_dsub
  - >> __aeabi_drsub
  - >> __aeabi_dadd
  - >> sqrt
  - >> __kernel_poly
  - >> __ARM_fpclassify
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_overflow
  - >> __mathlib_dbl_invalid
  - >> __mathlib_dbl_infnan2
  - >> __mathlib_dbl_divzero
  - >> __ARM_scalbn
  - >> __aeabi_cdrcmple
  - >> __set_errno
  - >> __aeabi_dmul
  [Called By]
  - >> BMP_UncompemstatedToTrue

  sqrt (Thumb, 76 bytes, Stack size 24 bytes, sqrt.o(i.sqrt))
  [Stack]

  - Max Depth = 64
  - Call Chain = sqrt ⇒ _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> pow

  _get_lc_numeric (Thumb, 44 bytes, Stack size 8 bytes, lc_numeric_c.o(locale$$code))
  [Stack]

  - Max Depth = 8
  - Call Chain = _get_lc_numeric
  [Calls]
  - >> strcmp
  [Called By]
  - >> __rt_lib_init_lc_numeric_2

  _get_lc_ctype (Thumb, 44 bytes, Stack size 8 bytes, lc_ctype_c.o(locale$$code))
  [Stack]

  - Max Depth = 8
  - Call Chain = _get_lc_ctype
  [Calls]
  - >> strcmp
  [Called By]
  - >> __rt_lib_init_lc_ctype_2
  [Address Reference Count : 1]
  - rt_ctype_table.o(.text)

  __aeabi_d2f (Thumb, 0 bytes, Stack size 32 bytes, d2f.o(x$fpl$d2f))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_d2f
  [Called By]
  - >> BMP_UncompemstatedToTrue
  - >> ADXL345_GetValue
  - >> Convert_BH1750
  - >> SHT2x_CalcRH
  - >> SHT2x_CalcTemperatureC

  _d2f (Thumb, 98 bytes, Stack size 32 bytes, d2f.o(x$fpl$d2f), UNUSED)
  [Calls]

  - >> __fpl_fretinf
  - >> __fpl_dnaninf

  __aeabi_dadd (Thumb, 0 bytes, Stack size 16 bytes, daddsub_clz.o(x$fpl$dadd))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_dadd
  [Called By]
  - >> SHT2x_CalcTemperatureC
  - >> __kernel_poly
  - >> __mathlib_dbl_infnan2
  - >> pow

  _dadd (Thumb, 332 bytes, Stack size 16 bytes, daddsub_clz.o(x$fpl$dadd), UNUSED)
  [Calls]

  - >> _dsub1
  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __fpl_dcheck_NaN1 (Thumb, 10 bytes, Stack size 0 bytes, dcheck1.o(x$fpl$dcheck1))
  [Calls]

  - >> __fpl_return_NaN
  [Called By]
  - >> __ARM_scalbn

  __fpl_dcmp_Inf (Thumb, 24 bytes, Stack size 0 bytes, dcmpi.o(x$fpl$dcmpinf), UNUSED)
  [Called By]

  - >> _dcmple

  __aeabi_ddiv (Thumb, 0 bytes, Stack size 32 bytes, ddiv.o(x$fpl$ddiv))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_ddiv
  [Called By]
  - >> BMP_UncompemstatedToTrue
  - >> Convert_BH1750
  - >> __mathlib_dbl_invalid
  - >> __mathlib_dbl_divzero
  - >> pow

  _ddiv (Thumb, 552 bytes, Stack size 32 bytes, ddiv.o(x$fpl$ddiv), UNUSED)
  [Calls]

  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __aeabi_i2d (Thumb, 0 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt))
  [Called By]

  - >> BMP_UncompemstatedToTrue
  - >> pow

  _dflt (Thumb, 46 bytes, Stack size 0 bytes, dflt_clz.o(x$fpl$dflt), UNUSED)

  __aeabi_cdcmple (Thumb, 0 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf), UNUSED)

  _dcmple (Thumb, 120 bytes, Stack size 32 bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Calls]

  - >> __fpl_dcmp_Inf
  - >> __fpl_dnaninf

  __fpl_dcmple_InfNaN (Thumb, 0 bytes, Stack size unknown bytes, dleqf.o(x$fpl$dleqf), UNUSED)
  [Called By]

  - >> _drcmple

  __aeabi_dmul (Thumb, 0 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_dmul
  [Called By]
  - >> BMP_UncompemstatedToTrue
  - >> ADXL345_GetValue
  - >> SHT2x_CalcRH
  - >> SHT2x_CalcTemperatureC
  - >> __kernel_poly
  - >> pow

  _dmul (Thumb, 332 bytes, Stack size 32 bytes, dmul.o(x$fpl$dmul), UNUSED)
  [Calls]

  - >> __fpl_dretinf
  - >> __fpl_dnaninf

  __fpl_dnaninf (Thumb, 156 bytes, Stack size 16 bytes, dnaninf.o(x$fpl$dnaninf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __fpl_dnaninf
  [Called By]
  - >> _ddiv
  - >> _dsub
  - >> _dadd
  - >> _d2f
  - >> _dsqrt
  - >> _dcmple
  - >> _dmul

  __fpl_dretinf (Thumb, 12 bytes, Stack size 0 bytes, dretinf.o(x$fpl$dretinf), UNUSED)
  [Called By]

  - >> _ddiv
  - >> _dadd
  - >> _f2d
  - >> _dmul

  __aeabi_cdrcmple (Thumb, 0 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_cdrcmple
  [Called By]
  - >> pow

  _drcmple (Thumb, 108 bytes, Stack size 16 bytes, drleqf.o(x$fpl$drleqf), UNUSED)
  [Calls]

  - >> __fpl_dcmple_InfNaN

  __aeabi_drsub (Thumb, 0 bytes, Stack size 8 bytes, daddsub_clz.o(x$fpl$drsb))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_drsub
  [Called By]
  - >> BMP_UncompemstatedToTrue
  - >> pow

  _drsb (Thumb, 22 bytes, Stack size 8 bytes, daddsub_clz.o(x$fpl$drsb), UNUSED)
  [Calls]

  - >> _dsub1
  - >> _dadd1

  _dsqrt (Thumb, 456 bytes, Stack size 24 bytes, dsqrt_noumaal.o(x$fpl$dsqrt))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ __fpl_dnaninf
  [Calls]
  - >> __fpl_dnaninf
  [Called By]
  - >> sqrt

  __aeabi_dsub (Thumb, 0 bytes, Stack size 32 bytes, daddsub_clz.o(x$fpl$dsub))
  [Stack]

  - Max Depth = 32
  - Call Chain = __aeabi_dsub
  [Called By]
  - >> SHT2x_CalcRH
  - >> pow

  _dsub (Thumb, 464 bytes, Stack size 32 bytes, daddsub_clz.o(x$fpl$dsub), UNUSED)
  [Calls]

  - >> _dadd1
  - >> __fpl_dnaninf

  __aeabi_f2d (Thumb, 0 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2d
  [Called By]
  - >> BMP180_test
  - >> ADXL345_GetValue
  - >> Convert_BH1750
  - >> SHT20_test
  - >> SHT2x_CalcRH
  - >> SHT2x_CalcTemperatureC

  _f2d (Thumb, 86 bytes, Stack size 16 bytes, f2d.o(x$fpl$f2d), UNUSED)
  [Calls]

  - >> __fpl_fnaninf
  - >> __fpl_dretinf

  __aeabi_f2uiz (Thumb, 0 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_f2uiz
  [Called By]
  - >> SHT2x_MeasureHM

  _ffixu (Thumb, 62 bytes, Stack size 16 bytes, ffixu.o(x$fpl$ffixu), UNUSED)
  [Calls]

  - >> __fpl_fnaninf

  __aeabi_i2f (Thumb, 0 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$fflt))
  [Called By]

  - >> ADXL345_GetValue

  _fflt (Thumb, 48 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$fflt), UNUSED)

  __aeabi_ui2f (Thumb, 0 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu))
  [Called By]

  - >> Convert_BH1750
  - >> SHT2x_CalcRH
  - >> SHT2x_CalcTemperatureC

  _ffltu (Thumb, 38 bytes, Stack size 0 bytes, fflt_clz.o(x$fpl$ffltu), UNUSED)

  __fpl_fnaninf (Thumb, 140 bytes, Stack size 8 bytes, fnaninf.o(x$fpl$fnaninf), UNUSED)
  [Called By]

  - >> _ffixu
  - >> _f2d

  __fpl_fretinf (Thumb, 10 bytes, Stack size 0 bytes, fretinf.o(x$fpl$fretinf), UNUSED)
  [Called By]

  - >> _d2f

  _printf_fp_dec (Thumb, 4 bytes, Stack size 0 bytes, printf1.o(x$fpl$printf1))
  [Stack]

  - Max Depth = 320
  - Call Chain = _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec_real
  [Called By]
  - >> _printf_g
  - >> _printf_e
  - >> _printf_f

  __fpl_return_NaN (Thumb, 100 bytes, Stack size 0 bytes, retnan.o(x$fpl$retnan))
  [Calls]

  - >> __fpl_cmpreturn
  [Called By]
  - >> __fpl_dcheck_NaN1

  __ARM_scalbn (Thumb, 92 bytes, Stack size 0 bytes, scalbn.o(x$fpl$scalbn))
  [Calls]

  - >> __fpl_dcheck_NaN1
  [Called By]
  - >> __mathlib_dbl_underflow
  - >> __mathlib_dbl_overflow
  - >> pow

  __fpl_cmpreturn (Thumb, 48 bytes, Stack size 0 bytes, trapv.o(x$fpl$trapveneer))
  [Called By]

  - >> __fpl_return_NaN

  ### Local Symbols

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  _dadd1 (Thumb, 0 bytes, Stack size unknown bytes, daddsub_clz.o(x$fpl$dadd), UNUSED)
  [Called By]

  - >> _dsub
  - >> _drsb

  _dsub1 (Thumb, 0 bytes, Stack size unknown bytes, daddsub_clz.o(x$fpl$dsub), UNUSED)
  [Called By]

  - >> _drsb
  - >> _dadd

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  _fp_digits (Thumb, 428 bytes, Stack size 96 bytes, _printf_fp_dec.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _btod_emul
  - >> _btod_ediv
  - >> _btod_d2e
  - >> _btod_etento
  - >> _ll_udiv10
  [Called By]
  - >> _printf_fp_dec_real

  ### Undefined Global Symbols