                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:3497313
Balance, indicates the remaining weight of filament in the 3D printer by cmachado is licensed under the Creative Commons - Attribution - Non-Commercial license.
http://creativecommons.org/licenses/by-nc/3.0/

# Summary

End your headaches, know in real time how much filaments you still have, know before printing whether that remaining filaments will be enough to print that piece, do not waste your time watching your print. Use this balance to give the information you need.
My facebook:https://www.facebook.com/cm3dtecnologia


# Print Settings

Printer: Sethi3D S3
Rafts: No
Supports: Yes
Resolution: 0.2mm
Infill: 20%
Filament_brand: 3DLAB
Filament_color: Black
Filament_material: PLA

Notes: 
Parts bpf3d_1 and bpf3d_2 must be printed with at least 20% infill, other parts may be printed with 10% infill, speed 65mm/min.

# Post-Printing

![Alt text](https://cdn.thingiverse.com/assets/f8/cf/d2/25/75/b2.PNG)
design of the assembled filament holder

![Alt text](https://cdn.thingiverse.com/assets/13/6c/ab/27/27/multif.png)
Multifunction shield, used to make the filament scale.

![Alt text](https://cdn.thingiverse.com/assets/63/5d/bd/8c/cb/uno.jpg)
Arduino Uno R3, used to make the filament scale.

![Alt text](https://cdn.thingiverse.com/assets/97/67/36/f3/ef/hx711.jpg)
HX711 Module, used to make the filament scale.

![Alt text](https://cdn.thingiverse.com/assets/62/9b/82/52/d9/celula.jpg)
5Kgs. Load Cell 75 milímeter, used to make the filament scale.

## List of materials for mounting the filament scale

- Print Filament Suport.
- Load Cell - 5Kgs. 75 milimeter.
- Arduino Uno R3.
- HX711 WFX, Module.
- Multifunction Shield.
- 04 Screws M4 x 25 mm.
- 08 flat washers M4.
- 04 pressure washers M4.
- 03 Screws M6 x (depending on where it will be fixed, greater than 20 mm).
- 03 flat washers M6.
- 03 pressure washers M6.
- 03 screw nuts M6.
- 4 way cable with awg shield # 26, (the length depends on the distance of the filament suport and the electronic assembly).
- The firmware of the filament balance can be purchased, just send a request through the email below, after the acquisition you will receive all the information of assembly and calibration.
e-mail: eletroncard@gmail.com

<iframe src="//www.youtube.com/embed/cUZTiQ-0PaQ" frameborder="0" allowfullscreen></iframe>