CONFIG_BT_NIMBLE_LOG_LEVEL_ERROR=y
CONFIG_BT_ENABLED=y
CONFIG_BT_NIMBLE_ENABLED=y
CONFIG_BT_CONTROLLER_ENABLED=y

CONFIG_BT_NIMBLE_SVC_GAP_DEVICE_NAME="MPY ESP32"

CONFIG_BT_NIMBLE_MAX_CONNECTIONS=4

# Put NimBLE on core 1, and for synchronisation
# with the ringbuffer and scheduler MP needs to be on the same core.
# MP on core 1 prevents interference with WiFi for time sensitive operations.
# Only on: ESP32, ESP32S2, ESP32S3
CONFIG_BT_NIMBLE_PINNED_TO_CORE_0=n
CONFIG_BT_NIMBLE_PINNED_TO_CORE_1=y
CONFIG_BT_NIMBLE_PINNED_TO_CORE=1

# Increase NimBLE task stack size from the default, because Python code
# (BLE IRQ handlers) will most likely run on this task.
CONFIG_BT_NIMBLE_TASK_STACK_SIZE=6144

# The MicroPython NimBLE bindings do not currently support dynamic NimBLE
# state, so disable it.
CONFIG_BT_NIMBLE_STATIC_TO_DYNAMIC=n
